Firmware Release Date: 2008-10-27
Firmware File: 2.0

Release Notes - Latest changes:

New modems:
# Alcatel One Touch X030
# Kyocera iBurst
# Novatel Wireless MC990D
# Novatel Wireless MCD3000
# Novatel Wireless (Verizon) USB727
# Quanta MU-Q101
# ZTE MF628+

New features:
# SMS Mailbox! (see setup video)
Check the list of modems which support this feature. You can send/receive SMS messages using the UMR. Also check if your SIM card supports SMS!
# Connection Tracker.
Checks the status of your internet connection and allows your UMR to take different routes of action in case of a disconnect. The UMR can reconnect, restart or automatically fail-over to a secondary interfaces (WAN port). You can define which interface, be it USB or WAN port will be primary or secondary.
# Ethernet WAN port.
This interface is now enabled for DHCP and Static IP addressing.
# WPA2 Enterprise.
Allows you to use RADIUS on the backend for WLAN authentication.
# GUI cleanup and rearrangement.

Upgrade Procedure:
1) Download the UMR20.zip
2) Unzip the UMR20.zip
3) Turn off your UMR.
4) Unplug the USB modem.
5) Turn on the UMR without USB modem inserted.
6) Log into the web interface of your UMR.
7) Go to Upgrade->HTTP Upgrade page.
8) Browse for the firmware file ("UMR20.bin") you have downloaded and unzipped off this website and select to upgrade.
9) Upgrade time is 3 minutes.